Hollow Clock

# Introduction

## Hollow Clock V New Software

This clock is based on the plans in Thingiverse. It is sold under license from the designer. I have, however, modified the software. The software now has a serial menu system that can be used to fine tune the clock’s accuracy and several other settings. I also changed the software to use the µSecond (microsecond) counter for more accuracy. The original code used the µSecond counter multiplied by 1000 to give µSeconds, but this of course doesn’t really increase the accuracy since the counter only reads mSeconds. In addition to this the code did not handle the counter overflow that happens about every 49 days. This caused a gain of up to a minute each time the overflow happened.

## Starting the Clock

The best way to start and set the clock to the correct time is to disconnect the USB C connector from the clock, set the hands to the correct time, and then plug in the USB C connector. Follow these steps to start the clock.

* Remove the rotor assembly by lifting it from the base.
* Move the clock hands to the correct time, perhaps the next minute.
* Replace the rotor assembly on the base while preventing the hands from moving.
* When the time (using an accurate clock, like a cell phone) matches the clock hands start the clock by connecting the USB C connector.

# Serial Port Menu System

## USB Connection to Computer

The clock must be connected to the computer to use the menu system. A USB C to A or C type connector may be used. The PC must be running some serial port software, such as SSCOM PuTTY or similar. The Arduino IDE is an excellent choice, it is free and easy to install. Enable the serial port monitor and a section of the IDE will display the text coming from the clock. The serial port is set to 9600 baud, 8 bits, no parity, 1 stop bit.

### Using PuTTY on Windows

Download and install PuTTY from here: [Download PuTTY: latest release (0.81)](https://www.chiark.greenend.org.uk/~sgtatham/putty/latest.html) or from the Windows Store.

The actual serial port for the clock will be needed. It can be found by running Windows “Device Manager” and opening the Ports section. The clock will be a USB Serial Device. Remember the name inside (). COM13 in this case.

Start PuTTY and select “Serial” as shown. Enter the com port name in the “Serial Line” field.

A screenshot of a computer

Description automatically generatedA screenshot of a computer

Description automatically generated

Press the “Open” button and the PuTTY window will open.

A screenshot of a computer

Description automatically generated

Clock commands can be entered using the keyboard. The enter key sends the command to the clock. The menu will be displayed again with any changed values. Entering a blank line just displays the menu. Every minute the clock will write a line showing the time that the clock has been running. This number is useful when calibrating the clock to keep more exact time.

## Received Data

Every minute a line will be sent from the clock to the serial port. This information is useful for calibrating the clock and setting certain other values.

Here is a sample line.

run time: 4 minutes = 0.07 Hours

The minutes and hours values are how long the clock has been running. The hours value is the same as the minutes divided by 60 and is used for the ‘F’ command to calibrate the clock.

## The Menu

The menu is displayed after entering ‘?’ or a blank line in the serial terminal software. Each command is a single character, some of which require additional information after the command.

------ Current Settings ------

Firmware version : 1.01

uSeconds calibrate per minute : -16635 or -23.95 sec/day

Wait/Run State : Running

Stepper Delay (mSec) : 2

Test Mode : Off

Reverse Motor : No

--- Commands ---

+<n> : Advance n minutes

-<n> : Reverse n minutes

A<n> : Adjust Minute Position (+/- 256 is a full minute)

W : Wait, toggle running state of clock

C<n> : Calibrate uSeconds per minute, is default, change as needed, +speeds up, -slows down

F<sec> <hours> : Figure correction using seconds and hours (floats), e.g. F -2.5 24.0 if 2 seconds slow per day

S<n> : Set stepper motor delay, default is 6, range 2 to 120

T : Test mode (enter anything while running to stop)

R : Reverse motor setting

Command?

The first part of the menu shows some current values. The last part lists the available commands with short descriptions. Note that this clock was running too fast. The -16635 was used to slow it down.

### Commands

#### +<n>

The integer <n> is used to advance the clock by that many minutes. E.g. +5 will move the clock forward by 5 minutes.

#### -<n>

The integer <n> will move the clock backwards by that many minutes.

#### A<n>

This value is used to adjust the minute pointer by small increments, so it lines up with the minute marks exactly. Both positive and negative values may be entered. If a negative value is entered the clock will move backwards and forwards again to take up the gear drive slack for more accuracy.

#### W

This command makes the clock stop. It is useful if you want to start the clock at a chosen exact time. Set the hands to the desired time and when the time is reached press ‘W’ and enter on the serial monitor program to start the clock running again.

#### C<n>

This command is used to adjust the running speed of the clock in µSeconds per minute. Positive values make the clock run faster and negative values make it run slower. This value can be calculated from monitoring the clock run for several days. Note that the F command is easier to use and will calculate the correct value to use.

#### F<sec> <hour>

This command will calculate the correct speed adjustment from the number of seconds per hour that the clock is fast or slow. Both numbers are entered as floating point (decimal) numbers. Seconds can be positive or negative. Negative indicates that the clock is running slow. The most accurate values are produced by monitoring the clock for longer periods of time, at least 12 hours, but several days is even better. As an example, if the clock loses 10.5 seconds in 2 days the correction would be entered as “F 10.5 48”. Using the log time on a serial monitor is the easiest way to measure how much is gained or lost, but noting the exact start and times of the watch period is also possible by watching when the status lines are printed each minute.

#### S<n>

S is used to set the stepper motor stepping delay. Weaker motors might need longer delays, or you might just like the different sound of slower or faster stepping.

#### T

This command toggles test mode. When test mode is on the clock runs continuously. This can test the servo and gears to make sure it rotates freely. Pressing any key and enter will stop the test mode and return to normal running.

#### R

The ‘R’ command is used to reverse the servo. This is needed when chosen servo runs in the opposite direction. It only needs to be set once, unless you want your clock to run backwards of course!